(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(uuid "e8ea0e98-76fb-4fc6-b23e-90888600fedf")
	(paper "A5")
	(title_block
		(title "EL223FP4L1")
		(date "2025-05-08")
		(rev "1")
		(company "Boles & Walker")
		(comment 1 "OUTPUT GAIN")
	)
	(lib_symbols
		(symbol "Custom:ADA4692-2"
			(pin_names
				(offset 0.127)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 2.54 6.35 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
				)
			)
			(property "Value" "ADA4692-2"
				(at 2.54 3.81 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
				)
			)
			(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
				(at -3.302 -6.35 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4691-2_4691-4_4692-2_4692-4.pdf"
				(at 5.588 10.16 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "Dual Low Noise, Precision, Rail-to-Rail Output, JFET Op Amp, SOIC-8"
				(at 0.508 -9.144 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "ki_keywords" "dual opamp"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "ADA4692-2_1_1"
				(polyline
					(pts
						(xy 5.08 0) (xy -5.08 5.08) (xy -5.08 -5.08) (xy 5.08 0)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -7.62 2.54 0)
					(length 2.54)
					(name "+"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin input line
					(at -7.62 -2.54 0)
					(length 2.54)
					(name "-"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 7.62 0 180)
					(length 2.54)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(symbol "ADA4692-2_2_1"
				(polyline
					(pts
						(xy 5.08 0) (xy -5.08 5.08) (xy -5.08 -5.08) (xy 5.08 0)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -7.62 2.54 0)
					(length 2.54)
					(name "+"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "5"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin input line
					(at -7.62 -2.54 0)
					(length 2.54)
					(name "-"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "6"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin output line
					(at 7.62 0 180)
					(length 2.54)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "7"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(symbol "ADA4692-2_3_1"
				(pin power_in line
					(at 0 7.62 270)
					(length 3.81)
					(name "V+"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "8"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin power_in line
					(at 0 -7.62 90)
					(length 3.81)
					(name "V-"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "4"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:R_Potentiometer_US"
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "RV"
				(at -4.445 0 90)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "R_Potentiometer_US"
				(at -2.54 0 90)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Footprint" ""
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "Potentiometer, US symbol"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_keywords" "resistor variable"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_fp_filters" "Potentiometer*"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "R_Potentiometer_US_0_1"
				(polyline
					(pts
						(xy 0 2.54) (xy 0 2.286)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.286) (xy 1.016 1.905) (xy 0 1.524) (xy -1.016 1.143) (xy 0 0.762)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0.762) (xy 1.016 0.381) (xy 0 0) (xy -1.016 -0.381) (xy 0 -0.762)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -0.762) (xy 1.016 -1.143) (xy 0 -1.524) (xy -1.016 -1.905) (xy 0 -2.286)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -2.286) (xy 0 -2.54)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.143 0) (xy 2.286 0.508) (xy 2.286 -0.508) (xy 1.143 0)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 2.54 0) (xy 1.524 0)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_Potentiometer_US_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 3.81 0 180)
					(length 1.27)
					(name "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:R_US"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.54 0 90)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "R_US"
				(at -2.54 0 90)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Footprint" ""
				(at 1.016 -0.254 90)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "Resistor, US symbol"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "R_US_0_1"
				(polyline
					(pts
						(xy 0 2.286) (xy 0 2.54)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.286) (xy 1.016 1.905) (xy 0 1.524) (xy -1.016 1.143) (xy 0 0.762)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0.762) (xy 1.016 0.381) (xy 0 0) (xy -1.016 -0.381) (xy 0 -0.762)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -0.762) (xy 1.016 -1.143) (xy 0 -1.524) (xy -1.016 -1.905) (xy 0 -2.286)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -2.286) (xy 0 -2.54)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_US_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 99.06 71.12)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "44680ec5-2a3e-4d88-b277-f2ff281bb45e")
	)
	(junction
		(at 121.92 54.61)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "7690d4e9-bb1b-493a-b1f5-5071a050ce72")
	)
	(junction
		(at 85.09 71.12)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "cc38a2f8-1639-4d5d-bd05-6de043ddece2")
	)
	(wire
		(pts
			(xy 85.09 44.45) (xy 85.09 48.26)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "1effaa2b-f99b-45f7-a7a6-fff32057c701")
	)
	(wire
		(pts
			(xy 99.06 57.15) (xy 101.6 57.15)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "23ea1311-80dc-456c-947c-d29c53e75aba")
	)
	(wire
		(pts
			(xy 121.92 71.12) (xy 121.92 54.61)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "34d64e41-dd59-4221-b024-d47665e014da")
	)
	(wire
		(pts
			(xy 121.92 54.61) (xy 129.54 54.61)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "3557f91f-faf4-48e1-888a-25f70f4f6632")
	)
	(wire
		(pts
			(xy 88.9 52.07) (xy 101.6 52.07)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "44fb37e0-e8e6-4041-a8fd-d428c3cbc423")
	)
	(wire
		(pts
			(xy 88.9 71.12) (xy 85.09 71.12)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "5115e97a-c0f1-4af4-88a1-631cb1cdab8c")
	)
	(wire
		(pts
			(xy 85.09 73.66) (xy 85.09 71.12)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "53eebce3-1999-41ef-b85f-fac70d8908c0")
	)
	(wire
		(pts
			(xy 78.74 44.45) (xy 85.09 44.45)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "87921b5b-c240-4f6b-b7d7-e6c6fb7209e0")
	)
	(wire
		(pts
			(xy 99.06 71.12) (xy 106.68 71.12)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "93d2d676-23ae-4181-95ea-11871719e6f4")
	)
	(wire
		(pts
			(xy 116.84 54.61) (xy 121.92 54.61)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "b77bcc1e-fad7-4585-8cef-5b935cdedb68")
	)
	(wire
		(pts
			(xy 96.52 71.12) (xy 99.06 71.12)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "c0aa92f6-f391-446b-9b52-4fc05aecca2b")
	)
	(wire
		(pts
			(xy 99.06 71.12) (xy 99.06 57.15)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "cff051d8-669c-4229-b068-bd812f5efd8d")
	)
	(wire
		(pts
			(xy 85.09 55.88) (xy 85.09 71.12)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "e82cd769-0582-4125-8981-71cf08a2c046")
	)
	(wire
		(pts
			(xy 114.3 71.12) (xy 121.92 71.12)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "e8c818ba-df62-4ba4-81bd-7430db22376e")
	)
	(global_label "VREF"
		(shape input)
		(at 85.09 73.66 270)
		(fields_autoplaced yes)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify right)
		)
		(uuid "20590858-c840-4c0c-86f1-9d99785982f1")
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 85.09 81.2414 90)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
				(hide yes)
			)
		)
	)
	(hierarchical_label "IN"
		(shape input)
		(at 78.74 44.45 180)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify right)
		)
		(uuid "145b7da1-30ef-44cc-a22c-a1ad5541e4d3")
	)
	(hierarchical_label "OUT"
		(shape output)
		(at 129.54 54.61 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left)
		)
		(uuid "ec7290fd-8b11-41b3-b8cb-cba5066f869c")
	)
	(symbol
		(lib_id "Custom:ADA4692-2")
		(at 109.22 54.61 0)
		(unit 2)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "59108bf8-6413-479a-90ba-385cd30e3342")
		(property "Reference" "U2"
			(at 109.22 44.45 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "ADA4692"
			(at 109.22 46.99 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 105.918 60.96 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4691-2_4691-4_4692-2_4692-4.pdf"
			(at 114.808 44.45 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Dual Low Noise, Precision, Rail-to-Rail Output, JFET Op Amp, SOIC-8"
			(at 109.728 63.754 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Sim.Library" "ada4692.sub"
			(at 109.22 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Sim.Name" "ADA4692-2"
			(at 109.22 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Sim.Device" "SUBCKT"
			(at 109.22 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Sim.Pins" "1=AOUT 2=AIN- 3=AIN+ 4=V- 5=BIN+ 6=BIN- 7=BOUT 8=V+"
			(at 109.22 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Part" "ADA4692-2ARZ"
			(at 109.22 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "22b8fae4-4cb1-475c-9f39-9b48ef7641d6")
		)
		(pin "4"
			(uuid "55c50349-5036-4cd2-9dd3-1130c47ac190")
		)
		(pin "5"
			(uuid "774e2dc1-a4ef-4a73-aed6-415511917893")
		)
		(pin "3"
			(uuid "9d36396e-fd95-4542-bb3e-c47c141b2080")
		)
		(pin "1"
			(uuid "01b42cf3-cf6b-4714-961b-5eb616e8aea9")
		)
		(pin "6"
			(uuid "ece5e20c-f5fa-4680-a393-b7f4c6093cc5")
		)
		(pin "7"
			(uuid "5376b1ff-54ce-4480-8a59-24e9dc5745e5")
		)
		(pin "8"
			(uuid "7095b578-3b86-4a9c-ab9d-c355a4252925")
		)
		(instances
			(project "ece223_project"
				(path "/3a60b8c4-9b6a-45e3-8d5f-2fa80fee2396/1f3891d7-9ed5-413e-b758-2e8f45955b50"
					(reference "U2")
					(unit 2)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_Potentiometer_US")
		(at 85.09 52.07 0)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "78db22f2-47ae-4d7e-a67e-26665d34e16a")
		(property "Reference" "RV6"
			(at 82.55 50.8 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
		)
		(property "Value" "10k"
			(at 82.55 53.34 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
		)
		(property "Footprint" "Custom:Potentiometer_Bourns_PTV09A-1_Single_Vertical"
			(at 85.09 52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/54/ptv09-777818.pdf"
			(at 85.09 52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Potentiometer, US symbol"
			(at 85.09 52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Sim.Device" "R"
			(at 85.09 52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Sim.Type" "POT"
			(at 85.09 52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Sim.Pins" "1=r0 2=wiper 3=r1"
			(at 85.09 52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Sim.Params" "pos=0.75"
			(at 85.09 52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Part" "PTV09A-4020U-B103"
			(at 85.09 52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "b143581d-ad60-4aa2-9af0-417e548a3869")
		)
		(pin "3"
			(uuid "baf78f2d-0527-4ada-a927-e8b145d8dff9")
		)
		(pin "1"
			(uuid "b3b8fc39-0bb5-4861-8c39-5e5392d35052")
		)
		(instances
			(project ""
				(path "/3a60b8c4-9b6a-45e3-8d5f-2fa80fee2396/1f3891d7-9ed5-413e-b758-2e8f45955b50"
					(reference "RV6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_US")
		(at 92.71 71.12 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "a87c4466-b97b-49f6-972e-0a8733c8b65c")
		(property "Reference" "R23"
			(at 92.71 64.77 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "10k"
			(at 92.71 67.31 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 92.964 70.104 90)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "~"
			(at 92.71 71.12 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor, US symbol"
			(at 92.71 71.12 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Part" ""
			(at 92.71 71.12 90)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "17d4b3b5-9d40-4ed7-b852-12f334f8d761")
		)
		(pin "2"
			(uuid "41ae0255-5897-4eb4-be38-066044fe31f1")
		)
		(instances
			(project ""
				(path "/3a60b8c4-9b6a-45e3-8d5f-2fa80fee2396/1f3891d7-9ed5-413e-b758-2e8f45955b50"
					(reference "R23")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R_US")
		(at 110.49 71.12 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "b34cccc6-0850-4ae0-9681-a854e214d449")
		(property "Reference" "R24"
			(at 110.49 64.77 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "30k"
			(at 110.49 67.31 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 110.744 70.104 90)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://static6.arrow.com/aropdfconversion/e88ae8119cc3549cbba033af6c2c6bd3b2796839/1088fileversion.pdf"
			(at 110.49 71.12 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor, US symbol"
			(at 110.49 71.12 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Part" "ERJ-P06F3002V"
			(at 110.49 71.12 90)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "9c737f48-ec89-4e29-8d19-4fd6bb7362d1")
		)
		(pin "2"
			(uuid "0f167025-c3d4-4ec8-9193-615f11a09576")
		)
		(instances
			(project "ece223_project"
				(path "/3a60b8c4-9b6a-45e3-8d5f-2fa80fee2396/1f3891d7-9ed5-413e-b758-2e8f45955b50"
					(reference "R24")
					(unit 1)
				)
			)
		)
	)
)
