(footprint "Potentiometer_Bourns_PTV09A-1_Single_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Potentiometer, vertical, Bourns PTV09A-1 Single, http://www.bourns.com/docs/Product-Datasheets/ptv09.pdf")
	(tags "Potentiometer vertical Bourns PTV09A-1 Single")
	(property "Reference" "RV1"
		(at 2.5 -8.5 180)
		(layer "F.SilkS")
		(uuid "d1378ba2-a30c-4816-8dae-b1520fbbf045")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "10k"
		(at 6.05 5.15 180)
		(layer "F.Fab")
		(uuid "6b3324d4-6b5f-4e48-8e1e-ca88bf2638a2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://www.mouser.com/datasheet/2/54/ptv09-777818.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ea03a3b2-41a4-4626-8814-c669b45a5103")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Potentiometer, US symbol"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a7bec42f-9a80-41e3-8ba8-8f6e7c79da5d")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Device" "R"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6b426efd-7f2e-40c2-aa9f-5c58c3fa830b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Type" "POT"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "cf6ca8bd-cd55-4077-8990-2db3919a9d73")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Pins" "1=r0 2=wiper 3=r1"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fbc96e06-fb09-4512-9592-55165b593f55")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Params" "pos=0.75"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a479d875-9747-4fd8-830d-73237deda31d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start 0.88 -7.47)
		(end 0.88 -5.871)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f2ed8abb-b40c-4a28-9f9a-ce23d0fa002e")
	)
	(fp_line
		(start 0.88 -7.47)
		(end 4.745 -7.47)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "661b3312-fe2c-4c3f-85d7-2e57539c47b4")
	)
	(fp_line
		(start 0.88 -4.129)
		(end 0.88 -3.37)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0cc48537-82f6-4de4-bfbf-1f68d05e16d2")
	)
	(fp_line
		(start 0.88 -1.629)
		(end 0.88 -0.87)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "80bbca26-f4e8-44fa-9b39-508ea5078828")
	)
	(fp_line
		(start 0.88 0.87)
		(end 0.88 2.47)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "496d676c-e536-47d5-827f-9248677fc2a7")
	)
	(fp_line
		(start 0.88 2.47)
		(end 4.745 2.47)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5ff1c542-0b3e-49c2-89ce-730181a4b650")
	)
	(fp_line
		(start 9.255 -7.47)
		(end 13.12 -7.47)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c7ec986d-6d4d-4d41-a412-0a5f10169254")
	)
	(fp_line
		(start 9.255 2.47)
		(end 13.12 2.47)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3fa0ebfb-7edd-4dc0-9f67-5042aec04d0c")
	)
	(fp_line
		(start 13.12 -7.47)
		(end 13.12 2.47)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "43806e99-e9b3-4cb4-bf0c-dba586336e4f")
	)
	(fp_line
		(start -1.15 -9.15)
		(end -1.15 4.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "dfbb3e60-b0ff-4ddf-95a8-0df777638509")
	)
	(fp_line
		(start -1.15 4.15)
		(end 13.25 4.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c7f66083-7888-4131-b383-78d34ebd0f29")
	)
	(fp_line
		(start 13.25 -9.15)
		(end -1.15 -9.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "3835727f-9799-495a-9d0f-398586cd4aa9")
	)
	(fp_line
		(start 13.25 4.15)
		(end 13.25 -9.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "43c4a09e-d3a8-4c65-a47e-0647491a3335")
	)
	(fp_line
		(start 1 -7.35)
		(end 1 2.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a3215d61-5c2d-44e8-9b60-58c6f71f3592")
	)
	(fp_line
		(start 1 2.35)
		(end 13 2.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c7638f80-e483-46a2-b1d3-5a28ce3b4f45")
	)
	(fp_line
		(start 13 -7.35)
		(end 1 -7.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b94afbc1-7b67-405c-bedf-f70f5af572a5")
	)
	(fp_line
		(start 13 2.35)
		(end 13 -7.35)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "66205ba6-d11a-464a-a924-300d8708e0c6")
	)
	(fp_circle
		(center 7 -2.5)
		(end 10 -2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "5ee6a02c-72c4-421a-be22-837fd9f0e834")
	)
	(fp_text user "${REFERENCE}"
		(at 2 -2.5 90)
		(layer "F.Fab")
		(uuid "6e66ebc8-c4d5-4f41-944f-971fde56f09c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at 7 -6.9)
		(size 4 4)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(uuid "228757f1-5e32-431b-90bf-27043e8a7902")
	)
	(pad "" np_thru_hole circle
		(at 7 1.9)
		(size 4 4)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(uuid "ecf46eaa-3ef7-4fe7-8022-ce828b4e5696")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "576d2a0d-1612-4252-8b26-27fd484bac76")
	)
	(pad "2" thru_hole circle
		(at 0 -2.5)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "abbd5b33-4d3a-4c12-a0da-434288423ecf")
	)
	(pad "3" thru_hole circle
		(at 0 -5)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2f84022d-9fb0-46ba-b5f8-4e757bcc44a7")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/PTV09A-4020U-B103.stp"
		(offset
			(xyz 7 2.5 6.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 -0 -90)
		)
	)
)
