(footprint "Jack_3.5mm_CUI_SJ1-3523N_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TRS 3.5mm, horizontal, through-hole, https://www.cuidevices.com/product/resource/pdf/sj1-352xn.pdf")
	(tags "TRS audio jack stereo horizontal")
	(property "Reference" "J2"
		(at -5.5 -8.5 180)
		(layer "F.SilkS")
		(uuid "0c654f8b-fa4f-47a2-81a2-43caaa61be90")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "AudioJack3"
		(at 0 -10 180)
		(layer "F.Fab")
		(uuid "dd034ac8-f201-4128-b362-c848c78d5c58")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9a94e79e-5e61-400c-83b8-a82d62cd2de3")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Audio Jack, 3 Poles (Stereo / TRS)"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "87ca7c44-3ec5-4baa-9158-905fb8814c6b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole exclude_from_pos_files)
	(fp_line
		(start -6 -7.7)
		(end 6 -7.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2caaa4c9-2552-42c9-8efa-4823e8e3273a")
	)
	(fp_line
		(start -6 3.3)
		(end -6 -7.7)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6168cc15-9263-4691-9982-0cb27c754831")
	)
	(fp_line
		(start -4.5 3.3)
		(end -6 3.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5e4ff711-0fc5-448b-a847-e4a3fea586a8")
	)
	(fp_line
		(start -4.5 4.25)
		(end -4.5 3.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4b06cb62-39cc-4494-8c23-7538cdcb1a30")
	)
	(fp_line
		(start -3 4.25)
		(end -4.5 4.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7eec701f-b98b-423c-bc24-5acb8fba801b")
	)
	(fp_line
		(start 4.5 3.3)
		(end 4.5 4.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "74ccfd81-e7cf-4eb4-a5c3-065bcb3fe8b9")
	)
	(fp_line
		(start 4.5 4.25)
		(end 3 4.25)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2ac0e0f7-992e-489d-866a-531554202f44")
	)
	(fp_line
		(start 6 -7.7)
		(end 6 3.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4e51d02d-c9c8-43cc-9533-95b284d4f22d")
	)
	(fp_line
		(start 6 3.3)
		(end 4.5 3.3)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f8328b14-c32f-4c98-8b2d-ecd3f71e4ac0")
	)
	(fp_line
		(start -2.2 3.5)
		(end -2.2 4.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "1a0a125d-2f9e-4f3d-8ec0-9ecbca0e72d5")
	)
	(fp_line
		(start -2.2 4.5)
		(end -6.25 4.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "cbe7658e-daf1-47c4-b9e8-520028d31236")
	)
	(fp_line
		(start 1.8 3.1)
		(end -1.8 3.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "bfd8b164-af69-4d94-9a60-cc85cd8acf8b")
	)
	(fp_line
		(start 2.2 3.5)
		(end 2.2 4.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "73d5260c-f456-466c-8c75-2f026f251f44")
	)
	(fp_line
		(start 2.2 4.5)
		(end 6.25 4.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "917e2030-c454-43c6-87a0-07c8b88861b0")
	)
	(fp_arc
		(start -2.2 3.5)
		(mid -2.082843 3.217158)
		(end -1.8 3.1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "9e1a8a33-8233-4abe-a3ba-a6b830ef1ba4")
	)
	(fp_arc
		(start 1.8 3.1)
		(mid 2.082843 3.217157)
		(end 2.2 3.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "eb0995bb-e678-4b76-8456-79056a51cc93")
	)
	(fp_line
		(start -6.25 -7.95)
		(end -6.25 4.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "f7c2dd8a-1687-4734-91d1-4dfb7034f7c3")
	)
	(fp_line
		(start -6.25 4.75)
		(end -3.25 4.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "63562dd3-f19b-48fe-9912-83c21a31173b")
	)
	(fp_line
		(start -3.25 4.75)
		(end -3.25 6.55)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "53cd6ca8-9049-4dde-a527-e45c9992f246")
	)
	(fp_line
		(start -3.25 6.55)
		(end 3.25 6.55)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "66071f1e-b04f-49dc-99fc-112775de4666")
	)
	(fp_line
		(start 3.25 4.75)
		(end 6.25 4.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "8f313e63-61ed-48a7-b525-151726762e88")
	)
	(fp_line
		(start 3.25 6.55)
		(end 3.25 4.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1fdee5e4-d354-4a89-a782-922f99f0e291")
	)
	(fp_line
		(start 6.25 -7.95)
		(end -6.25 -7.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "99b2d1bc-2d92-46bd-9ad4-a4b8c5d2b637")
	)
	(fp_line
		(start 6.25 4.5)
		(end 6.25 -7.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "01ecbe1f-b510-4450-8a7b-a5ff96f3be8e")
	)
	(fp_line
		(start 6.25 4.75)
		(end 6.25 4.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "bfbdbfd5-18dd-4d16-8ae7-db7a4fc2250f")
	)
	(fp_line
		(start -6 -7.7)
		(end 6 -7.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2b0ed5ae-9ef1-49c6-b870-50a36d11edb4")
	)
	(fp_line
		(start -6 3.3)
		(end -6 -7.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "0725ffe5-df0b-4701-8f35-03d8576d35e0")
	)
	(fp_line
		(start -4.5 3.3)
		(end -6 3.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "31437e38-2c3c-4611-a389-8d47159f22f9")
	)
	(fp_line
		(start -4.5 4.5)
		(end -4.5 3.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "627f591d-0721-4c96-95ed-d8436d1de7c0")
	)
	(fp_line
		(start -4.5 4.5)
		(end -3 4.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e7a935b2-6890-444a-9191-8315d1a3863d")
	)
	(fp_line
		(start -3 4.5)
		(end -3 6.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "525e5d32-e41b-485d-a969-c3759af256bd")
	)
	(fp_line
		(start -3 6.3)
		(end 3 6.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4e4878bb-834b-4523-89f4-8f366cd67ff1")
	)
	(fp_line
		(start 3 4.5)
		(end 3 6.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ee43d5a4-51d1-4bf6-80b4-2fc050730633")
	)
	(fp_line
		(start 4.5 3.3)
		(end 6 3.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7075e3ee-249b-4a64-b9df-19fd19567562")
	)
	(fp_line
		(start 4.5 4.5)
		(end 3 4.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1a4392cc-55e5-48e9-9cf6-f721b6cb2ca8")
	)
	(fp_line
		(start 4.5 4.5)
		(end 4.5 3.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e882e3b6-4f8d-4411-8a37-16a04ebbe7d7")
	)
	(fp_line
		(start 6 3.3)
		(end 6 -7.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "74201cde-46d1-4161-95b1-40aad522b14e")
	)
	(fp_text user "PCB edge"
		(at 0 5.5 180)
		(unlocked yes)
		(layer "Dwgs.User")
		(uuid "6603ea05-abec-4c3a-be70-d0b3c84a8d32")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 -1.5 180)
		(layer "F.Fab")
		(uuid "8c0c633e-b05d-4fc8-b3bf-07db7b17d22b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at -5 0)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(uuid "e6224198-ac11-4f62-bf91-8032e22b87ab")
	)
	(pad "" np_thru_hole circle
		(at -5 2.5)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(uuid "9a8acccb-5f0e-4165-ba3a-267584607e89")
	)
	(pad "" np_thru_hole circle
		(at 0 -5)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(uuid "05569bc5-3ecf-416b-b82e-d5b5e46c5574")
	)
	(pad "" np_thru_hole circle
		(at 5 0)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(uuid "cb0bc6ed-43c4-4165-89f3-10bb650a041b")
	)
	(pad "" np_thru_hole circle
		(at 5 2.5)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(uuid "2e191cf7-e0e2-4715-bc0a-33183645d0ac")
	)
	(pad "R" thru_hole oval
		(at -5 -5)
		(size 1.2 2.2)
		(drill oval 0.4 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "3d7c16d9-41fc-4ed0-a02b-90aaff7df646")
	)
	(pad "S" thru_hole oval
		(at 0 0)
		(size 2.2 1.2)
		(drill oval 1.4 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "064127bf-3194-4932-a513-0f75ad34515b")
	)
	(pad "T" thru_hole oval
		(at 5 -5 180)
		(size 1.2 2.2)
		(drill oval 0.4 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a3dcf3d3-5f1d-4da2-9605-d277a906782f")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ1-3523N_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
